**48 V DC powered BLDC Motor based fans with feature for remote operation**

**Technical Specifications**

|  |  |  |  |
| --- | --- | --- | --- |
| **Parameter** | **Specifications** | | |
| Type of fan | External rotor | | |
| Type of motor | PM BLDC | | |
| Fan size (Sweep) | 1200 ±5 mm | | |
| Nominal Operating Voltage | 48 V DC | | |
| Operating Voltage Range | 45-52 V DC | | |
| Power input | 30 W Max | | |
| Max Speed | 300 – 320 RPM | | |
| Air delivery at max speed | 200-210 m3/min | | |
| Motor controller | Sensor less control strategy | | |
| ON/OFF and speed control operation | With built-in remote (IR) Sensor for external remote control | | |
| Multiple speed settings | From 180 RPM to max speed in near equal steps from remote | | |
| Starting | Fan shall start and run at 45 V to 52 V DC | | |
| Start up at all speeds | Smooth starting with a maximum of 180 degree (mechanical) reverse rotation, if any. | | |
| Memorising last set speed | Fan controller shall be capable of running at the last set speed, at the time of Power ON | | |
| Insulation resistance | 5 M Ohm @ 600 V DC | | |
| Winding Temperature rise | 70 ◦ C | | |
| Type of blades | Aluminium sheet | | |
| Protection features | Blocked Blade, Reverse polarity, Over voltage and Over Current | | |
| Operating noise at at full speed | 65 dBA | | |
| No load operating noise | 52 dBA | | |
| Motor construction | Totally enclosed type | | |
| Corrosion resistance | Motor body and blades shall be corrosion resistant | | |
| Safe operation temperature | 50 ◦ C | | |
| Max humidity | 90 % Rh | | |
| Other fan accessories | Standard down rod, canopy and shackle clip | | |
| Safety features | Compliance to mechanical safety of fan suspension system (clamp and down rod) | | |
| **Remote control signals, commands and codes** | | | |
| Communication Protocol | | NEC derived custom protocol | |
| Carrier Frequency | | 38 ± 1 kHz | |
| Operating distance (line of sight) | | 5 m | |
| Feedback signal to user | | Light signals to user for 2s whenever remote is operated | |
| Control signals | | Command | Hex Codes |
| Fan ON or OFF | | F\_ON\_OFF | 0x00FF42BB |
| Fan speed increase | | F\_UP | 0x00FF52AA |
| Fan speed decrease | | F\_DN | 0x00FF7888 |
| **Code description** | | | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Command** | **Hex Code** | **Binary Codes (32 bits)** | **Reversal of binary digits in**  **Hex Code** | **Decimal**  **notation of the Code** |
| F\_ON\_OFF | 0x00FF42BB | 0b 0000 0000 1111 1111 0100 0010 1011 1011 | DD42FF00 | 3712155392 |
| F\_UP | 0x00FF52AA | 0b 0000 0000 1111 1111 0101 0010 1010 1010 | 554AFF00 | 1430978304 |
| F\_DN | 0x00FF7888 | 0b 0000 0000 1111 1111 0111 1000 1000 1000 | 111EFF00 | 287244032 |
| **Data reception** | | As per NEC protocol for communication | | |
| 1. **(i) Total length of the data reception in one cycle in 32 bits.**  * Logical '0' – a 562.5µs high signal followed by a 562.5µs low signal, with a total   time of 1.125ms   * Logical '1' – a 562.5µs high signal followed by a 1.6875ms low signal, with a total time of 2.25ms.   **(ii) Start sequence:** A high signal of 9ms followed by a low signal of 4.5ms and thus making a total time of 13.5ms; bit sequence is modulating signal. | | | | |