**Specifications for Laser Beam Profiler**

The specifications required are as follows:

1. Resolution: 700\*500 pixels (minimum)

2. Cell size (m\*m): 10\*10 (maximum)

3. Active area (mm\*mm):  6\*4.5 (minimum)

4. Wavelength range (m):  0.4 -1.6

5. Damage threshold (W/sq. cm): 50

6. Frame rate: 25 fps with full resolution (minimum)