**SPECIFICATION FOR STANDING INFORMATION KIOSKS**

**(Quantity – 4 Nos.)**

|  |  |  |
| --- | --- | --- |
| **S.NO** | **COMPONENTS** | **REQUIRED SPECIFICATION** |
| **1.** | **CPU** | * Intel Atom D425@ 1.80 GHz (or) * Intel Atom D525@1.80 GHz * Intel Atom D2550 @ 1.86GHz * Intel Atom N2800 @ 1.86GHz. * Intel Atom E3845@ 1.91 GHz * Intel Atom Z2760 @1.60 GHz * Intel Core2 Duo P7700 @ 1.80 GHz * Intel Core2 Duo SL9400 @1.86 GHz * Intel Core2 Duo T5550 @ 1.83 Ghz * Intel Core2 Duo T5600 @ 1.83 GHz * Intel Core2 Duo T5670 @ 1.86 GHz |
| **2.** | **MEMORY** | Required > = 2GB RAM |
| **3.** | **HARD DISK DRIVE (HDD)** | Required >= 80 GB |
| **LED DISPLAY** | | |
| **4.** | **SIZE** | Required >= 24 inch TFT LCD |
| **5.** | **RESOLUTION** | 1280 X 1024 @ 75Hz |
| **6.** | **BRIGHTNESS** | 250 cd/m2 |
| **7.** | **PROTECTIVE LAYER** | Vandal-proof with **6**mm antiglare and overlay Protection. |
| **8.** | **SPECIFIC REQUIREMENT FOR KIOSK**   * Screen with unbreakable glass for outdoor usage. * 24 x 7 running capability * Extra USB ports for mouse and keyboard * UPS (Minimum back up time of 2 hours) * Provision for Internet wireless modem/GPRS connectivity * Remote Management Software * Steel Enclosure with security features * Protection from sun, rain and dust for outdoor usage * Should be able to handle temperature variation from 100C TO 550C. * Easy lock access to inner hidden connector ports. * Ergonomically designed for all ages and heights of people. * 24 x 7 product service/support. | |
| **9** | **COLOUR** | Dark colour for outdoor usage |
| **10** | **I/O CONNECTIVITY** | USB PORT Required 4,  Serial Required 1,  Ethernet Port Required 1 |
| **11** | **COOLING FAN** | As per requirement for outdoor usage |

* 2 year warranty required. 10% of the total cost would be with-held and will be released on half-yearly basis depending on the service provided.
* AMC after the warranty period should be quoted separately on a quarterly basis, and will be released at the end of the period based on service provided.